ALTO LINE

In both traditional and trendy newly build and renovation projects large glazed sections and terrace windows are often used to optimise natural lighting and thus limiting the open wall space. With the Alto Line Henrad offers you the ideal solution. When combining the Alto Line with the Everest Line 8 and Compact Line models a light and spacious feeling is created throughout the home.

Product: the decorative vertical radiator with a centre connection and a stylised front

Finishing: decorative stylised front and side panels

Also supplied: wall brackets, ETA safety screws and plugs, screws, plugs, air vent, blind plugs and installation instructions

Connections: 4 x ½” female connection (centre connection included)

Lugs: no lugs

Packaging: Every radiator is sturdily packaged in high-quality cardboard and wrapped in plastic. The radiator’s characteristics are shown on the label: type – height – length.

Warranty: 10 years, as long as the installation instructions have been followed and Henrad’s warranty conditions have been met.

Paint process: All radiators are degreased, phosphated, cataphoretically primed and powder-coated in Henrad white 9016 as standard.

Colours: Henrad white 9016 + 35 different Henrad colours and about 200 RAL-colours are possible

Max. operating pressure: 10 bar (tested to 13 bar)

Max. operating temperature: 110 °C

Conformity: in accordance with EN442

Quality assurance: NF

Types: 11 | 20 | 21 | 22

Heights: 1.600 | 1.800 | 2.000 | 2.200 mm

Lengths: 300 | 400 | 500 | 600 | 700 mm

Depths: 49 | 79 | 79 | 102 mm