ALTO SWING

Elegant and decorative is how we can best describe the Alto Swing. The Alto Swing not only charms with its beautiful rounded contours, it also provides heating performance that exceeds expectations. With the wide availability of colours you can decide to have the Alto Swing blend into your interior or have it stand out conspicuously on its own merits.

Product: the decorative vertical radiator with a centre connection, a minimum distance to the wall and round curves

Finishing: completely smooth, rounded design

Also supplied: wall brackets, ETA safety screws and plugs, screws, plugs, air vent, blind plugs and installation instructions

Connections: 4 x ½” female connection (centre connection included)

Lugs: no lugs

Packaging: Every radiator is sturdily packaged with protective foam-filled bags, in high-quality cardboard and wrapped in plastic. The radiator’s characteristics are shown on the label: type – height – length.

Warranty: 10 years, as long as the installation instructions have been followed and Henrad’s warranty conditions have been met.

Paint process: All radiators are degreased, phosphated, cataphoretically primed and powder-coated in Henrad white 9016 as standard.

Colours: Henrad white 9016 + 35 different Henrad colours and about 200 RAL-colours are possible

Max. operating pressure: 10 bar (tested to 13 bar)

Max. operating temperature: 110 °C

Conformity: in accordance with EN442

Types: 21 | 22

Heights: 1.820 | 2.020 mm

Lengths: Type 21: 504 | 604 | 704 mm
Type 22: 527 | 627 | 727 mm

Depths: 96 | 119 mm