ALTO TANGO

The plain, sleek design means this radiator matches any interior in any living style. The front curves round nicely into the side panels in one flowing seamless form. A range of colours allows you to go that one step further in fully adapting the Alto Tango to match your interior requirements.

Product: the decorative vertical radiator with a centre connection, a minimum distance to the wall and a neat angular look

Finishing: completely smooth, angled design

Also supplied: wall brackets, ETA safety screws and plugs, screws, plugs, air vent, blind plugs and installation instructions

Connections: 4 x ½” female connection (centre connection included)

Lugs: no lugs

Packaging: Every radiator is sturdily packaged with protective foam-filled bags, in high-quality cardboard and wrapped in plastic. The radiator’s characteristics are shown on the label: type – height – length.

Warranty: 10 years, as long as the installation instructions have been followed and Henrad’s warranty conditions have been met.

Paint process: All radiators are degreased, phosphated, cataphoretically primed and powder-coated in Henrad white 9016 as standard.

Colours: Henrad white 9016 + 35 different Henrad colours and about 200 RAL-colours are possible

Max. operating pressure: 10 bar (tested to 13 bar)

Max. operating temperature: 110 °C

Conformity: in accordance with EN442

Types: 21 | 22

Heights: 1.820 | 2.020 mm

Lengths: 510 | 610 mm

Depths: 96 | 119 mm