ARNO SINGLE E

An attractive white electric tubular towel radiator, offering timeless elegance and functional energy efficiency. A perfect choice for bathrooms, the Arno Single E electric towel radiator features a simple and elegant steel tube on tube design that provides adequate and convenient hanging space for towels.

Product: Electric vertical round tube-on-tube design radiator

Pre-installed: Prefilled with heating liquid, equipped with a thermostat and a 1,2 m insulated cable with plug.

Also supplied: Brackets, screws, plugs and manual

Control: Operated via integrated thermostat with weekly programming, open window detection, presence detection and boost function.

Packaging: Every radiator is sturdily packaged in high-quality cardboard and wrapped in plastic. The radiator’s characteristics are shown on the label: electric power – height – length.

Warranty: 10 years for the radiator and 2 years for the electrical components, as long as the installation instructions have been followed, Henrad’s warranty conditions have been met and the radiator is installed outside the splash area.

Paint process: All radiators are degreased, phosphated and powder-coated.

Colour: Traffic White

Conformity: EcoDesign 2018 (EU Regulation 2015/1188)

Technical data: Voltage 230V ~50Hz, IP34, Class II

Heights: 1.195 | 1.523 | 1.810 mm

Number of tubes: 23 | 29 | 36

Lengths: 500 | 600 mm

Depth: 56 mm

Output: 500 | 700 | 1.000 W

Tubes: horizontal, O-section, diameter 22 mm

Collectors: vertical, O-section, diameter 35 mm