COMPACT PLAN

The Compact Plan differs from an ordinary compact radiator because it comes complete with a flat front and close-fitting side panels and decorative upper grille. Use the Compact Plan in combination with the Everest Plan and Alto Plan models to create an uniform sleek look.

Product: the decorative encased panel radiator with a flat front plate

Finishing: decorative flat front with upper grille and side panels

Also supplied: VDI brackets with anti-lift (type Monclac), screws, plugs, air vent, blind plug and installation instructions

Connections: 4 x ½” female connection

Lugs: 2 pairs of mounting lugs up to 1.600 mm and 3 pairs from 1.800 mm

Packaging: Every radiator is sturdily packaged in high-quality cardboard and wrapped in plastic. The radiator’s characteristics are shown on the label: type – height – length.

Warranty: 10 years, as long as the installation instructions have been followed and Henrad’s warranty conditions have been met.

Paint process: All radiators are degreased, phosphated, cataphoretically primed and powder-coated in Henrad white 9016 as standard.

Colours: Henrad white 9016 + 35 different Henrad colours and about 200 RAL-colours are possible

Max. operating pressure: 10 bar (tested to 13 bar)

Max. operating temperature: 110 °C

Conformity: in accordance with EN442

Quality assurance: NF

Types: 11 | 21 | 22 | 33

Heights: 300 | 400 | 500 | 600 | 700 | 900 mm

Lengths: 400 – 2.000 mm

Depths: 63 | 79 | 102 | 160 mm