NAVALE

The Navale is an oil filled radiator made with slim and compact vertical flat columns.

Product: Electric horizontal radiator

Pre-installed: Prefilled with oil, equipped with a thermostat and a 1,2 m insulated cable with plug.

Also supplied: Brackets, screws, plugs, manual and remote control.

Control: Operated via an integrated thermostat with weekly programming and open window detection.

Packaging: Every radiator is sturdily packaged in high-quality cardboard and wrapped in plastic. The radiator’s characteristics are shown on the label: electric power – height – length.

Warranty: 10 years for the radiator and 2 years for the electrical components, as long as the installation instructions have been followed, Henrad’s warranty conditions have been met and the radiator is installed outside the splash area.

Paint process: All radiators are degreased, phosphated, primed and powder-coated.

Colours: Traffic white or anthracite grey

Conformity: EcoDesign 2018 (EU Regulation 2015/1188)

Technical data: Voltage 230 V ~ 50 Hz, IP24, Class II

Height: 580 mm

Lengths: 440 | 520 | 760 | 920 mm

Depth: 90 mm

Output: 700 l 1.000 | 1.500 | 1.800 W