OCEANUS E-VENTO

The Oceanus E-VENTO is an electric radiator with integrated blower unit that provides extra heat emission (950 watt).

After the simple installation and insertion of the plug, the radiator is ready for use and you can enjoy a pleasant heat within a few minutes.

Product: electric classic bathroom radiator with blower

Pre-mounted: Pre-filled with heating fluid. Equipped with thermostat, 950 watt PTC blower and 1,2 m insulated cable with plug.

Also supplied: including brackets, screws, plugs and manual.

Control: Control via integrated thermostat with automatic self-learning weekly programming, open window detection, presence detection and boost function. RF receiver for optional remote control.

Packaging: Every radiator is sturdily packaged in high-quality cardboard and wrapped in plastic. The radiator’s characteristics are shown on the label: type – height – length.

Warranty: 10 years for the radiator and 2 years for the electrical components, as long as the installation instructions have been followed, Henrad’s warranty conditions have been met and the radiator is installed outside the splash area.

Paint process: All radiators are degreased, phosphated and powder-coated in Henrad white 9016 as standard.

Colours: Henrad white 9016 + 35 different Henrad colours and about 200 RAL-colours are possible

Conformity: EcoDesign 2018 (EU Regulation 2015/1188)

Technical data: Voltage 220-240V ~50Hz, IPX4, Class II

Heights: 775 | 1.181 | 1.411 | 1.763 mm

Number of tubes: 16 | 24 | 28 | 36

Lengths: 495 | 585 mm

Output: 1.350 | 1.550 | 1.650 | 1.850 | 1.950 W

Tubes: horizontal, O-section, diameter of 22 mm