RAGGIO

The Raggio provides natural, evenly distributed heat thanks to the transmission of infrared rays.

Product: Electric infrared panel

Pre-installed: 1,2 m insulated cable with plug

Also supplied: Brackets, screws, plugs and manual

Control: The IR-panel is delivered without thermostat. It must be installed with an intelligent third party electric smart plug. The control options of the plug must comply with EcoDesign 2018 (EU Regulation 2015/1188).

Packaging: Every IR-panel is sturdily packaged in high-quality cardboard. The IR-panel’s characteristics are shown on the label: electric power - height – length.

Warranty: 10 years for the IR-panel and 2 years for the electrical components, as long as the installation instructions have been followed, Henrad’s warranty conditions have been met and the IR-panel is installed outside the splash area.

Paint process: All IR-panels are degreased, phosphated and powder-coated

Colours: Traffic white or anthracite grey

Technical data: Voltage 230V ~50Hz, IP34, Class II

Heights: 1.218 | 1.540 | 1.740 mm

Lengths: 530 | 580 | 630 mm

Depth: 50 mm

Output: 500 | 700 | 1.000 W