VENICE

The fashionable solution for your bathroom.

Product: Venice, vertical flat tube-on-tube design radiator

Also supplied: 4 brackets, screws, plugs, air vent, blind plugs and installation instructions

Connections: 4 x ½” female connection (centre connection included)

Packaging: Every radiator is sturdily packaged in high-quality cardboard and wrapped in plastic. The radiator’s characteristics are shown on the label: height – length.

Warranty: 10 years, as long as the installation instructions have been followed, Henrad’s warranty conditions have been met and the radiator is installed outside the splash area.

Paint process: All radiators are degreased, phosphated and powder-coated in Henrad white 9016 as standard.

Colours: Henrad white 9016 + 35 different Henrad colours and about 200 RAL-colours are possible

Max. operating pressure: 4 bar (tested to 5,2 bar)

Max. operating temperature: 95 °C

Conformity: in accordance with EN442

Heights: 1.186 | 1.511 | 1.771 mm

Number of tubes: 16 | 20 | 24

Lengths: 450 | 600 mm

Tubes: horizontal, 60 x 10 mm flat section

Collector: vertical, O-section, diameter 38 mm