VERONA VERTICAL

The super slim radiator.

Product: Verona Vertical, vertical flat tube-on-tube design radiator

Also supplied: 4 white brackets (in chrome for any other radiator colour), anti-lift clip, bracket hiders, screws, plugs, design air vent and blind plug, blind plugs and installation instructions

Connections: 4 x ½” female connection (centre connection included)

Packaging: Every radiator is sturdily packaged in high-quality cardboard and wrapped in plastic. The radiator’s characteristics are shown on the label: height – length.

Warranty: 10 years, as long as the installation instructions have been followed, Henrad’s warranty conditions have been met and the radiator is installed outside the splash area.

Paint process: All radiators are degreased, phosphated and powder-coated in Henrad white 9016 as standard.

Colours: Henrad white 9016 + 35 different Henrad colours and about 200 RAL-colours are possible

Max. operating pressure: 4 bar (tested to 5,2 bar)

Max. operating temperature: 95 °C

Conformity: in accordance with EN442

Heights: 1.600 | 1.800 | 2.000 mm

Number of tubes: 6 | 8 | 10 | 12

Lengths: 408 | 538 | 668 | 798 mm

Tubes: vertical, 60 x 10 mm flat section

Collector: horizontal, O-section, diameter 38 mm