ALTO PLAN

The Alto Plan combines a sleek and decorative appearance and is perfect for applications where wall space is at a premium. This radiator can be perfectly combined with the Everest Plan 8 and Compact Plan models to provide a modern design and consistent look throughout your home.

Product: the decorative vertical radiator with a centre connection and a flat front

Finishing: decorative flat front and side panels

Also supplied: wall brackets, ETA safety screws and plugs, screws, plugs, air vent, blind plugs and installation instructions

Connections: 4 x ½” female connection (centre connection included)

Lugs: no lugs

Packaging: Every radiator is sturdily packaged in high-quality cardboard and wrapped in plastic. The radiator’s characteristics are shown on the label: type – height – length.

Warranty: 10 years, as long as the installation instructions have been followed and Henrad’s warranty conditions have been met.

Paint process: All radiators are degreased, phosphated, cataphoretically primed and powder-coated in Henrad white 9016 as standard.

Colours: Henrad white 9016 + 35 different Henrad colours and about 200 RAL-colours are possible

Max. operating pressure: 10 bar (tested to 13 bar)

Max. operating temperature: 110 °C

Conformity: in accordance with EN442

Quality assurance: NF

Types: 11 | 20 | 21 | 22

Heights: 1.600 | 1.800 | 2.000 | 2.200 mm

Lengths: 300 | 400 | 500 | 600 | 700 mm

Depths: 49 | 79 | 79 | 102 mm